# Genesys Quality Management Suite 8.1.520 : Configuring the JTAPI Adapter

Created and last modified by

Navigate to Settings > Configuration > Protocol Adapters > JTAPI adapter.

The configuration of the JTAPI adapter includes the following parameters:

Application Communicator:

- Bind name: The registered name of JTAPI RMI service
- Registry address: The server where the RMI service runs

Provider Setting:

- CallManager: The IP address for CUCM
- Login name: The login name for CUCM
- Password: The login password

The login name and password must correspond to the login name and password created for the application's user in the CUCM to communicate with Call Recording.

Communication with Core:

- TCP port: the Core server communication port, for example, the port that the Core connects to.

To function correctly the JTAPI adapter must have correctly configured Drivers and Readers.

## Downloading JTAPI Library from CUCM

If JTAPI Service is selected during the configuration process then the configuration wizard will be prompted to download the JTAPI library from CUCM. If this wasn't done then it can be done manually by executing the following command via ssh under root account:

    /opt/callrec/bin/get-jtapi

Icon

Without the JTAPI library Call Recording cannot record calls using the JTAPI signaling protocol.