# Genesys Quality Management Suite 8.1.520 : Hardware Platforms and Sizes

This section gives examples of suitable available servers from several manufacturers.

## Sizes

For the following tables the definitions for the sizes are:

- Small: Small/remote sites (up to 100 calls).
  Distributed deployments – servers without storage (RS, DS, RTS).
- Medium: Medium size sites (up to 250 calls) – 2 servers.
  Distributed deployments – higher processing power demands – DS.
- Large: DB and Storage for Replay Servers.
  The difference between the Large and Medium size servers is just disk space (and/or SAN/NAS).

## Hardware Platforms

| Small | Medium | Large
--- | --- | --- | ---
HP | ProLiant DL320 G6 | ProLiant DL360 G7 | ProLiant DL380 G7 + StorageWorks D2600/D2700
IBM | IBM x3250 M3 | IBM x3550 M3 | IBM x3550 M3 + Storage DS3500
DELL | PowerEdge R310 | PowerEdge R510 | PowerEdge R710 + PowerVault MD3200
Cisco UCS C-series rack-mount | UCS C200 M2 Rack Svr, 1x E5620, 1x4GB, 1PS | UCS C210 M2 Rack Svr, 2x E5620, 4x4GB, 2PS | UCS C250 M2 Rack Svr, 2x X5650, 8x4 GB, 2 PS
Cisco UCS B-series blade | UCS B200 M2 Blade Server, 1x E5620, 1x4GB | UCS B200 M2 Blade Server, 2x E5620, 4x4GB | UCS B200 M2 Blade Server, 2x X5650, 4x8 GB

## HP Details

Small server – ProLiant DL320 G6

- Max. 1 CPU (2 or 4 core), max. 96GB RAM
- 2 NIC, 2 expansion slots
- Up to 4 LFF or 8 SFF SAS/SATA/SSD disks – up to 2.4TB – RAID10 with 600GB HDDs

Medium server – ProLiant DL360 G7

- Max. 2 CPU (2, 4 or 6 core), max. 192GB RAM
- 2 NIC, 2 expansion slots
- Up to 8 SFF SAS/SATA/SSD disks - up to 2.4TB – RAID10 with 600GB HDDs

Large server – ProLiant DL380 G7

- Max. 2 CPU (2, 4 or 6 core), max. 192GB RAM
- 2 NIC, 6 expansion slots
- Up to 16 SFF SAS/SATA/SSD disks (with optional 2nd drive cage) - up to 8.4TB – RAID5 with 600GB HDDs, but external NAS/SAN storage recommended.

## IBM Details

Small server – IBM System x3250 M3

- Max. 1 CPU (2 or 4 core), max. 32GB RAM
- 2 NIC, 2 expansion slots
- Up to 2 LFF or 4 SFF SAS/SATA/SSD disks – up to 1.2TB – RAID10 with 600GB HDDs

Medium server – IBM System x3550 M3

- Max. 2 CPU (2, 4 or 6 core), max. 192GB RAM
- 2 NIC, 2 expansion slots
- Up to 8 SFF SAS/SATA/SSD disks – up to 2.4TB – RAID10 with 600GB HDDs

Large server – IBM System x3630 M3

- Max. 2 CPU (2, 4 or 6 core), max. 96GB RAM
- 2 NIC, 3 expansion slots
- Up to 24 SFF SAS/SATA/SSD disks – up to 11TB – RAID5 with 500GB HDDs, but external NAS/SAN storage recommended

## Dell Details

Small server – PowerEdge R310

- Max. 1 CPU (2 or 4 core), max. 32GB RAM
- 2 NIC, 2 expansion slots
- Up to 4 LFF/SFF SAS/SATA/SSD disks – up to 1.2TB – RAID10 with 600GB HDDs

Medium server – PowerEdge R510

- Max. 2 CPU (4 or 6 core), max. 128GB RAM
- 2 NIC, 4 expansion slots
- Up to 14 SFF SAS/SATA/SSD disks – up to 7.2TB – RAID5 with 600GB HDDs

Large server – PowerEdge R710

- Max. 2 CPU (4 or 6 core), max. 192GB RAM
- 2 NIC, 4 expansion slots
- Up to 8 SFF SAS/SATA/SSD disks – up to 2.4TB – RAID10 with 600GB HDDs, but external NAS/SAN storage recommended.

## Attachments:

t25.png (image/png)